**Correcting the Hardness of Your Water**

The hardness level in hot tub water should always be

between 150 to 250 ppm.

The hardness level is determined by the amount of calcium in your water. It’s more common to have a low hardness level than a high one.

An improper hardness level can cause increased foaming, cloudy water, and if left uncorrected it can cause damage to your spas equipment and even create scaling on your spa shell surface.

HT Liquid Calcium is the easiest way to raise the hardness level in your hot tub and because it comes higher concentrate then most other brands, it does not require a lot to add in...